*************************
How to use the bootloader

First, download the Windows distribution of the PIC16F876 from http://www.workingtex.com/htpic.
Get it working, then substitute this DOS downloader for it.

The default options for the bootloader are 19200bps.

A sample command line would be, for 19200bps, serial port COM1:

c:\DOWNLDR -S19200 -PCOM1 TEST.HEX